Red led

Traffic light state

CRAETE button ISR TASK

CRAETE Pedestrian task

CRAETE TRAFFIC LIGHT CONTROL TASK

START

Wait for button press

set Pedestrian to walk

delay for Pedestrian to walk

set Pedestrian to not walk

Delay for red led

Red led

Delay for yellow led

Yellow led

Yellow led

Delay for Green led

Green led